**Input voltage, Vin** = 24V

**Switching frequency , Fs** = 100kHz

**Output voltage , Vo** = 20V

**Maximum output power, Pomax** = 60W ( 3A maximum output current)

**Imin** = 100mA (Rmax = 200ohm)

**Buck converter operational mode** = continuous conduction mode (CCM)